36'-0" = Proscenium width (also distance between legs) 48'-0" = Approx. usable width between fixed lighting booms 56'-0" = Approx. overall width wall to wall  
  
30'-0" = Depth from plaster line to upstage black scrim  
14'-0" = Proscenium opening height (16'-0" arch, less 2'-0" fixed border)   
  
18’0” = Height from stage floor to hanging grid.